Additional note for vendors with vehicles: Display vehicles and equipment exhibited inside the building, including any gas-powered items, must have gas caps taped or locked and batteries disconnected, and shall not be fueled in the building. Fuel in the fuel tank shall not exceed 1/4 of the tank capacity or 5 gallons, whichever is less. MSFC 314.4.